README TEXT  for  Soft synthesizer S-YXG50		        

This file contains the latest information,corrections and addendum's for 
your version of the program.
Read the following instruction before proceeding.

This Document contains the following:
1. Version Numbers
2. List of files
3. File Summary
4. Installing   Soft synthesizer S-YXG50
5. Uninstalling Soft synthesizer S-YXG50
6. Specifications
7. System requirements
8. XG HOME page


1. Version Numbers:  

2.00		SXGB.DLL  
2.00		SXGBVSWP.SYS 
2.00		SXGBSYS.DLL 
2.00		SXGCPL.CPL   
MU50 2MB	SXGBIN2.TBL
MU50 2MB	SXGWAVE2.TBL    
 

2. List of Files:

SXGB.DLL  	    80,384  07-10-97  15:46 
SXGBVSWP.SYS 	   596,992  07-10-97  15:52
SXGBSYS.DLL         38,912  07-10-97  15:48 
SXGCPL.CPL          75,264  07-10-97  15:47 
SXGBIN2.TBL        149,995  20-07-97  14:11 
SXGWAVE.TBL      2,092,994  19-07-96  21:19
Psapi.dll           18,192  26-11-96  12:00
OEMSETUP.INF           262  03-09-97  16:34

3. File Summary:

SXGB.DLL  	User mode driver.

VSWP.SYS	Kernel mode driver.

SXGBIN2.TBL     Wave parameter table 	

SXGWAVE2.TBL    Wave table  	
 
SXGBSYS.DLL 	SXG manager 
         
SXGCPL.CPL      Control Panel application

Psapi.dll	Process Status Helper provided from MicroSoft

OEMSETUP.INF	Windows NT installation file.  
                It will install the files, update the registry.




4.  Installing Soft synthesizer S-YXG50

Help Fille,MIDIfile Player and Driver data Installation

4.1.Insert the disk into the computer's disk drive.
4.2. Double-click on the "Setup.exe" file .
4.3. All files will be copied to YMAHA\SXG50 folder(Default setting)
	MIDI	MIDI files
	Driver	S-YXG50 Driver file

The SXG Driver Installation

4.5. S-YXG50 requires Hardware CODEC & driver. Before installing the SXG driver, 
     check your system.
4.6. Double click the Multimedia icon in the control panel and click on the Devices tab.
4.7. Press the ADD button. Select Unlisted or Updated Drivers and press OK.
4.8. A dialog box will appear and request the path of the location of the
    driver files. You may search this path by clicking the BROWSE button.
    ( Default folder is \Program files\YAMAHA\SXG50\Driver)
4.9. Another dialog box will appear with the SXG50 Driver label. Press OK to continue
   with the installation.
4.10. Windows NT may ask you to restart your system.  Even though it is not
   necessary to do so, we recommend that you click on the Restart Now
   button.

5.  Uninstalling Soft synthesizer S-YXG50

*********  Remarks!!! **********************************************
 Please run the uninstall program to remove the folder completely.
 Do not remove the S-YXG50 folder. 
********************************************************************
 
Use the following procedure if you wish to delete the S-YXG50 from your hard disk.

Help Fille,MIDIfile Player and Driver data Uninstallation 
5.1. Click the [Start] button, and go to [Programs (P)] >> [Yamaha SoftSynthesizer S-YXG50]
   and select [uninstall S-YXG50]. 
5.2.  After the program starts, follow the directions given on-screen.

The SXG Driver Uninstallation
 
5.3.  Double click the Multimedia icon in the control panel and click on
     the Devices tab.  Double click on the Audio Devices entry and then
5.4.  Select MIDI for S-YXG50 Driver. Press the REMOVE button.  
    Verify your decision by pressing the YES button of the REMOVE dialog box.
5.5. The System Setting Change dialog box will appear and ask you to
   restart Windows NT.  Press the Restart Now button.

6. Specifications

   	Tone Generation         : Wave Table
   	Number of Voices        : 676 Melody Voices + 42 SFX Voices+
                                  21 Drum/SFXKits
                                 (XGMODOE 480Melody Voices + 
                                  42 SFX Voices + 11 Drum/SFXKitsj    
   	Multi-timbral Parts     : 16
   	Maximum Polyphony       : 128 notes
   	Effect Processor        : 8 Chorus + 8 Reverb + 
                                  36 Variation Effect
   	Sampling Rate           : 44/ 22/ 11kHz 
   	Digital Dynamic Filter is included
   	Direct Sound (R) Support

7. Hardware Requirement
	CPU : MMX (TM)Technology Pentium(R) Processor 133MHz or higher
	System Memory : 16MB or over
	Operating Sysytem : Windows NT4.0 workstation
	Sound Function : 16bit Stereo Sound CODEC

8.  The XG home page

XG-related information is available from the Yamaha home pages:

http://www.yamaha.co.jp/english/xg/
http://www.yamaha.com
http://www.yamaha.co.uk

XG MIDI FILE
You can get various XG MIDI files from same WWWW.


NOTE:
* Soft Synthesizer is a trademark of the Yamaha Corporation. 
* Microsoft, Direct Sound and Windows are registered trademarks of the Microsoft Corporation. 
* Pentium and MMX are registered trademarks of Intel Corporation, 
* Company names and product names etc. in README.TXT are registered trademarks or trademarks
  of their respective owners. 

Copyright (C) 1996-1997 YAMAHA CORPORATION
All Rights Reserved

