                        3Com (R) Corporation
                    EtherDisk (R) Diskette for the
          3C90X EtherLink XL 10/100 / EtherLink XL  NIC Family
      NetWare 4.11 on Windows 95/98 Client Driver Installation Notes



Intranetware Client Version 2.5/3.0 Installation Tips
----------------------------------------------------

If you have problems with the installation of Client 32
contact your network administrator or Novell.
3Com does not recommend installing the ODI 32-bit driver
in Windows 95/98.

Here are some procedures in installing Intranetware Client 2.5/3.0.

1.If you have Windows 95/98 installed , proceed and install the 3C905B NIC
in your system. Refer to Win98.txt on this disk if needed.

2.Follow the recommended procedure and tips in installing the NIC. Make
sure that you have the default services and protocols installed. The
necessary NIC NDIS driver will be installed in your system by default.

3.Copy the Intranetware client install files to your hard drive. About 33MB
when downloaded from Novell's file site.

4.Run setup.exe from the intranetware client install file location.
If you have the files on CD run the setup.exe from the intranetware client
install file location on the CD.

5.Select Typical or Custom installation, then click on Install.

6.The install will now copy all the necessary files and remove existing
client services that is not needed. 

7. The install may ask for network parameter input, follow the screen
instructions as needed.

8.Reboot your system when prompted.

                                                   
         (%VER CLIENT32.TXT - Installation guide v4.0.2)
