|  | Specification

General Specification
1. | Scanning Method | CIS moving operation in scanning direction
2. | Scanning Width | 8.5 inch +/-3%
3. | Scanning Length | 11.7 inch +/- 3%
4. | Scanning Mode | Line-Art, Gray (True Gray, Red Gray, Green Gray, Blue Gray), Color mode (with ON/Off average mode selected by software)
5. | Optincal Resolution | 600 x 1200dpi / 300 x 600 dpi
6. | DPI Selection | 50 to 19200 dpi selected by software
7. | Interface | USB
8. | Contrast Control | Controlled by software with 256 steps ranged from 100%(Least)-0%(Default)-100%(Most)
9. | Exposure Time | 6ms x 3/line for 600-dpi color picture mode 6ms/line for 300-dpi black & white text mode
10. | Paper Size Limitation | Single page Paper length: 20mm to 297mm Paper width: 20mm to 216mm
11. | Color Depth | 48-bits
12. | Temperature | Storage: -10 to 70 Degree C Operation: 10 to 40 Degree C
13. | Humidity | Storage: 10 % to 90 % RH non-condensing Operation: 35 % to 80 % RH non-condensing
Regulation Requirement
Safety : UL 1950 cUL 1950 TUV/GS EN60950 C-Tick CNS EMI: FCC Part 15 Sub-Part J Class B CE Mark (ESD 8KV without error, 10KV without damage) CNS VCCI (optional)