
  ---------------------------------------
    CRYSTAL AUDIO DRIVER VERSION D2720   
             for Windows95
  ---------------------------------------
             RELEASE NOTES
  ---------------------------------------
               04-01-98
  ---------------------------------------


This Document contains the following:
    1.  WHQL certification information
    2.  List of files
    3.  Installing Crystal Audio Drivers
    4.  Uninstalling Crystal Audio Drivers
    5.  Copyright and Trademarks




1.  WHQL Ceritification Information (PC97)

    PART        MASTER ID     CERTIFICATION DATE
    ^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^^
    CS4235      5009          05-23-98
    CS4236B     5010          05-23-98
    CS4237B     4868          05-16-98
    CS4239      5008          05-26-98


    **  CERTIFIED CWDAUDIX.VXD  04-07-98 **


2.  List of Files:
    CWD3DSND EXE       206,848  04-01-98 12:27a
    CWDAUDIO BIN         8,676  04-01-98 12:27a
    CWDAUDIO DRV       173,472  04-01-98 12:27a
    CWDAUDIO INI           774  04-01-98 12:27a
    CWDAUDIO INF        28,725  04-01-98 12:27a
    CWDAUDIX VXD        91,176  04-07-98 12:27a
    CWDFM    DRV        21,808  04-01-98 12:27a
    CWDINIT  EXE        98,176  04-01-98 12:27a
    CWDJOY   VXD        10,133  04-01-98 12:27a
    CWDMIDI  VXD        14,494  04-01-98 12:27a
    CWDMIDI  DRV         9,952  04-01-98 12:27a
    CWDMIX   EXE       239,320  04-01-98 12:27a
    CWDPCPLE DLL        37,888  04-01-98 12:27a
    SETUP    EXE        79,872  04-01-98 12:27a


3.  Installing Crystal Audio Drivers
    1.	During the Windows95 boot procedure.  Insert the Crystal 
	Driver Disk.  Windows95 will detect the CS423x device.  Press the 
	NEXT button. The Crystal PnP Audio System CODEC driver will be found.
	Press the FINNISH button.

    2.	The operating system will prompt you to provide the Crystal 
	Driver Disk.  Please insert this disk and press the OK button to 
	continue.  Then type A:\ and press the OK button.

 
4.  Uninstalling or Updating Crystal Audio Drivers
    
    1. 	From Win95, run UNINSTAL.EXE located in the Crystal Driver Disk.  
	This application will do an automatic cleaning up of the Windows 95 
        Crystal Audio registry entries.  Many problems with reinstallation 
        occur because of existing registry entries from previous installations
        and because of the \WINDOWS\INF\OEMx.INF files.  After running 
        UNINSTAL.EXE, the various Crystal devices should not be listed in the 
        Device Manager window.  

    2. 	Restart your system.  If you want to remove or install any hardware, 
	select the SHUTDOWN option and turn off your PC.

    3.	Turn PC on.  Upon loading, Windows 95 will detect new hardware, create 
	an information database, and proceed with the installation of Crystal 
	device drivers (as described in the previous section)



5.  Copyright and Trademarks
    * All brands and product names noted herein are the property or trademarks
      of their respective holders.


  ---------------------------------------
     Cirrus Logic, 1998
  ---------------------------------------
