/*****************************************************************************
** Control file for Crystal Semiconductor audio driver & FM installation.
**
** Copyright (c) 1994 IBM Corporation.  All Rights Reserved
** Copyright (c) 1994-1998 Cirrus Logic Corporation.  All Rights Reserved
**
** Filename: CTRAUDFM.SCR.
** When copied to "control.scr", this file controls OS/2 multimedia
** installation program, minstall.exe.  This file controls the installation
** of Crystal Semiconductor wave audio and IBM OPL-3 (FM) device drivers.
*****************************************************************************/

package="Crystal Audio OS/2 Warp/Merlin Installation"
codepage=437
filelist="FILAUDFM.SCR"
groupcount=2
munitcount=1
medianame="Crystal Audio OS/2 Installation Diskette "

sourcedir="\\"= 0

destindir="\\MMOS2\\"          = 0
destindir="\\MMOS2\\DLL\\"     = 2
destindir="\\MMOS2\\MOVIES\\"  = 3
destindir="\\MMOS2\\INSTALL\\" = 4
destindir="\\MMOS2\\DSP\\"     = 5
destindir="\\MMOS2\\HELP\\"    = 7
destindir="\\MMOS2\\SOUNDS\\"  = 9
destindir="\\OS2\\BOOT\\"      = 10
destindir="\\OS2\\"            = 11

/* Base Group */
ssgroup=0
ssname="mmbase"
ssversion="1.1.3"
sstermdll="ITERM.DLL"
sstermdllentry="ITermEntry"

/* Audio Adapter Group                                                      */
/* Modify this group to describe your adapter by changing the following:    */
/*  ssgroup   - Change this number only if you add a new group.             */
/*  ssname    - Put your adapter's name here                                */
/*  ssversion - Put the version number of your device driver here           */
/*  sssize    - Put the total size (in KB) of your device driver(s), help   */
/*              file, GENIN.DLL, GENINMRI.DLL, & any other files you install*/
/*  ssdllinputparms - this must match the ID number used in cardinfo.dll    */
/*  ssicon    - The icon that MINSTALL uses for your driver                 */
/*  ssinich   - Uncomment this line if you are adding a MIDI Map Table      */

/* Crystal Semiconductor Audio */
ssgroup=10
ssname="Crystal Audio"
ssversion="2.02.0"
/* sssize field is used to calculate percent done indicator */
sssize=55
ssdll="CWINST.DLL"
ssdllentry="CWINSTENTRY"
ssdllinputparms="10"
sstermdll="CWINST.DLL"
sstermdllentry="CWINSTEXIT"
ssselect="YES"

/* IBM FM */
ssgroup=20
ssname="IBM OPL3 FM MIDI Synthesis"
ssicon="midiplay.ico"
ssversion="1.0.0"
sssize=31
ssdll="genin.dll"
ssdllentry="InitGenin"
ssdllinputparms="20"
sscoreqs=10
ssselect="YES"
