[Version]
Signature="$WINDOWS NT$"
ClassGuid={4D36E96C-E325-11CE-BFC1-08002BE10318}
Class=MEDIA
Provider=%CRYSTAL%

[SourceDisksNames]
1 = %DiskId%

[SourceDisksFiles]
cwbaudll.dll = 1
cwbaudio.sys = 1
joyport.dll  = 1
joyport.sys  = 1
csbase.dll   = 1
csbase.sys   = 1
cwbaudio.bin  = 1
cspnp.inf    = 1
CWB3DSnd.exe = 1

[DestinationDirs]
cwbaudlldll.CopyList = 11 ; DIRID_SYSTEM
cwbaudiosys.CopyList = 12 ; DIRID_DRIVERS
joyportdll.CopyList  = 11 ; DIRID_SYSTEM
joyportsys.CopyList  = 12 ; DIRID_DRIVERS
csbasedll.CopyList   = 11 ; DIRID_SYSTEM
csbasesys.CopyList   = 12 ; DIRID_DRIVERS
CWB3DSnd.CopyList    = 11 ; DIRID_SYSTEM

[Manufacturer]
%CSMfgName%=CrystalSemiconductor

[CrystalSemiconductor]
;
; NOTE:  We omit hardware IDs for each of these devices, so that the user will
;        be able to supply an OEM-supplied driver with fuller functionality at
;        the "Found New Hardware" popup.
;%*CSC0000.DeviceDesc%=CSC0000_Device,, *CSC0031
;
%*CSC0000.DeviceDesc%=CSC0000_Device,, *CSC0000
%*CSC0010.DeviceDesc%=CSC0010_Device,, *CSC0010
%*CSC0010.DeviceDesc%=CSC0010_Device,, *CSC0002
%*CSC0003.DeviceDesc%=CSC0003_Device,, *CSC0003
%*PNPB02F.DeviceDesc%=MSJSTICK,,       *CSC0001
;
;new Mahler IDs
;
%*CSC0000.DeviceDesc%=CSC0000_Device,, *CSC0100
%*CSC0010.DeviceDesc%=CSC0010_Device,, *CSC0110
%*CSC0003.DeviceDesc%=CSC0003_Device,, *CSC0103
%*PNPB02F.DeviceDesc%=MSJSTICK,,       *CSC0101


[CSC0000_Device.NT]
CopyFiles=cwbaudlldll.CopyList,cwbaudiosys.CopyList,CWB3DSnd.CopyList
AddReg=CSC0000.AddReg, CS423X.AddReg, CWB3DSnd.AddReg
DelReg=CSC0000.DelReg, CWB3DSnd.AddReg
Reboot

[CSC0010_Device.NT]
CopyFiles=csbasedll.CopyList,csbasesys.CopyList
AddReg=CSC0010.AddReg, CSBASE.AddReg
Reboot

[CSC0003_Device.NT]
;CopyFiles=mpu401dll.CopyList,mpu401sys.CopyList
;AddReg=CSC0003.AddReg, MPU401.AddReg
;Reboot

[MSJSTICK.NT]
CopyFiles=joyportdll.CopyList,joyportsys.CopyList
AddReg=MSJSTICK.AddReg
Reboot

; This service is to be added to the front of the Extended Base services group
[CSC0000_Device.NT.Services]
AddService = cwbaudio, 0x00000003, cwbaudio_Service_Inst

[CSC0010_Device.NT.Services]
AddService = csbase, 0x00000002, csbase_Service_Inst

[CSC0003_Device.NT.Services]
;AddService = mpu401, 0x00000002, mpu401_Service_Inst

[MSJSTICK.NT.Services]
AddService = joyport, 0x00000002, joyport_Service_Inst

[cwbaudio_Service_Inst]
DisplayName    = %cwbaudio.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 1                  ; SERVICE_SYSTEM_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\cwbaudio.sys
LoadOrderGroup = Extended Base

[csbase_Service_Inst]
DisplayName    = %csbase.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 1                  ; SERVICE_SYSTEM_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\csbase.sys
LoadOrderGroup = Base

[joyport_Service_Inst]
DisplayName    = %joyport.SvcDesc%
ServiceType    = 1                  ; SERVICE_KERNEL_DRIVER
StartType      = 1                  ; SERVICE_SYSTEM_START
ErrorControl   = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\joyport.sys
LoadOrderGroup = Base

[cwbaudlldll.CopyList]
cwbaudll.dll
cwbaudio.bin
midimap.cfg
cspnp.inf

[cwbaudiosys.CopyList]
cwbaudio.sys

[csbasedll.CopyList]
csbase.dll

[csbasesys.CopyList]
csbase.sys

[joyportdll.CopyList]
joyport.dll

[joyportsys.CopyList]
joyport.sys

[CWB3DSnd.CopyList]
CWB3DSnd.exe


[CS423X.AddReg]
HKR,Drivers\wave\cwbaudll.dll,Driver,,cwbaudll.dll
HKR,Drivers\midi\cwbaudll.dll,Driver,,cwbaudll.dll
HKR,Drivers\mixer\cwbaudll.dll,Driver,,cwbaudll.dll
HKR,Drivers\aux\cwbaudll.dll,Driver,,cwbaudll.dll
HKR,Drivers,SubClasses,,"wave,midi,aux,mixer"

[CSC0000.DelReg]
;Clear FM's MIDI mapping name and make sure possibly translated name is
;created fresh out of DLL resource. Otherwise NT40 reuse old one.
HKLM,SYSTEM\CurrentControlSet\Control\MediaResources\MIDI\cs32ba11.dll<0000>,,,
HKLM,SYSTEM\CurrentControlSet\Control\MediaResources\MIDI\cs32ba11.dll<0001>,,,
HKLM,SYSTEM\CurrentControlSet\Control\MediaResources\MIDI\cs32ba11.dll<0002>,,,
HKLM,SYSTEM\CurrentControlSet\Control\MediaResources\MIDI\cs32ba11.dll<0003>,,,
HKLM,SYSTEM\CurrentControlSet\Control\MediaResources\MIDI\cwbaudll.dll<0000>,,,
HKLM,SYSTEM\CurrentControlSet\Control\MediaResources\MIDI\cwbaudll.dll<0001>,,,
HKLM,SYSTEM\CurrentControlSet\Control\MediaResources\MIDI\cwbaudll.dll<0002>,,,
HKLM,SYSTEM\CurrentControlSet\Control\MediaResources\MIDI\cwbaudll.dll<0003>,,,
HKLM,SYSTEM\CurrentControlSet\Control\MediaResources\MIDI\mmdrv.dll<0000>,,,
HKLM,SYSTEM\CurrentControlSet\Control\MediaResources\MIDI\mmdrv.dll<0001>,,,
HKLM,SYSTEM\CurrentControlSet\Control\MediaResources\MIDI\mmdrv.dll<0002>,,,
HKLM,SYSTEM\CurrentControlSet\Control\MediaResources\MIDI\mmdrv.dll<0003>,,,


[CSC0000.AddReg]
HKR,Drivers\wave\cwbaudll.dll,Description,,%*CSC0000.DeviceDesc%
HKR,Drivers\midi\cwbaudll.dll,Description,,%V_INTERNAL%
HKR,Drivers\mixer\cwbaudll.dll,Description,,%*CSC0000.DeviceDesc%
HKR,Drivers\aux\cwbaudll.dll,Description,,%*CSC0000.DeviceDesc%
HKR,MIXER,WaveVolumeOffset,,48
HKR,MIXER,lLineVolume,,45874
HKR,MIXER,rLineVolume,,45874
HKR,MIXER,lDac2Volume,,42280
HKR,MIXER,rDac2Volume,,42280
HKR,MIXER,LineGang,,ON
HKR,MIXER,lMicVolume,,45874
HKR,MIXER,rMicVolume,,45874
HKR,MIXER,MicVolume,,45874
HKR,MIXER,MicGang,,ON
HKR,MIXER,lAuxInVolume,,45874
HKR,MIXER,rAuxInVolume,,45874
HKR,MIXER,AuxInGang,,ON
HKR,MIXER,lLoopBackInputVolume,,45874
HKR,MIXER,rLoopBackInputVolume,,45874
HKR,MIXER,LoopBackInputGang,,ON
HKR,MIXER,MonitorVolume,,42280
HKR,MIXER,MonitorMute,,ON
HKR,MIXER,MonitorMode,,Recording
HKR,MIXER,lMasterVolume,,45874
HKR,MIXER,rMasterVolume,,45874
HKR,MIXER,MasterMute,,OFF
HKR,MIXER,MasterGang,,ON
HKR,MIXER,lAuxVolume,,45874
HKR,MIXER,rAuxVolume,,45874
HKR,MIXER,AuxMute,,OFF
HKR,MIXER,AuxGang,,ON
HKR,MIXER,lAux2Volume,,42280
HKR,MIXER,rAux2Volume,,42280
HKR,MIXER,Aux2Mute,,OFF
HKR,MIXER,Aux2Gang,,ON
HKR,MIXER,lLineMixVolume,,42280
HKR,MIXER,rLineMixVolume,,42280
HKR,MIXER,LineMixMute,,OFF
HKR,MIXER,LineMixGang,,ON
HKR,MIXER,MonoVolume,,42280
HKR,MIXER,MonoMute,,ON
HKR,MIXER,MonoOutMute,,ON
HKR,MIXER,MicBoost,,OFF
HKR,MIXER,lLowPriMicVolume,,45874
HKR,MIXER,rLowPriMicVolume,,45874
HKR,MIXER,LowPriMicMute,,ON
HKR,MIXER,LowPriMicBoost,,ON
HKR,MIXER,lLowPriLineVolume,,45874
HKR,MIXER,rLowPriLineVolume,,45874
HKR,MIXER,lLowPriLoopBackInputVolume,,45874
HKR,MIXER,rLowPriLoopBackInputVolume,,45874
HKR,MIXER,lLowPriAuxInVolume,,45874
HKR,MIXER,rLowPriAuxInVolume,,45874
HKR,MIXER,lVirtMaster,,45874
HKR,MIXER,rVirtMaster,,45874
HKR,MIXER,VirtMasterMute,,OFF
HKR,MIXER,VirtMasterGang,,ON
HKR,MIXER,DisableKaraokeMode,,OFF
HKR,MIXER,KaraokeMode,,OFF
HKR,MIXER,SmartKaraokeMode,,ON
HKR,MIXER,ExternalXCTL0Enable,,0
HKR,MIXER,ExternalXCTL1Enable,,N
HKR,MIXER,SuspendXCTL0Value,,1
HKR,MIXER,SuspendXCTL1Value,,N
HKR,MIXER,ResumeXCTL0Value,,0
HKR,MIXER,ResumeXCTL1Value,,N

;------------------- control values for symmetrical mixer ----------
HKR,MIXER,InputSelection,,8
HKR,MIXER,LowPriInputSelection,,8
HKR,MIXER,lDacSERVolume,,45874
HKR,MIXER,rDacSERVolume,,45874
HKR,MIXER,DacSERMute,,ON
HKR,MIXER,lLine-inVolume,,45874
HKR,MIXER,rLine-inVolume,,45874
HKR,MIXER,Line-inInputMute,,ON
HKR,MIXER,Line-inOutputMute,,ON
HKR,MIXER,3DSpace,,32768
HKR,MIXER,3DCenter,,32768
HKR,MIXER,3DMute,,OFF
HKR,MIXER,Aux2InputMute,,OFF
HKR,MIXER,Aux1InputMute,,OFF
HKR,MIXER,LineInputMute,,OFF
HKR,MIXER,MicInputMute,,OFF
HKR,MIXER,MicOutputMute,,ON
HKR,MIXER,lWaveOutVolume,,42280
HKR,MIXER,rWaveOutVolume,,42280
HKR,MIXER,WaveOutMute,,OFF
HKR,MIXER,WaveInMute,,ON
HKR,MIXER,lSysVol,,42280
HKR,MIXER,rSysVol,,42280
HKR,MIXER,lWaveinMasterVolume,,36000
HKR,MIXER,rWaveinMasterVolume,,36000

;---------- added for volume table-driven method--------
HKR,MIXER,AnalogGainTable,,%AnalogGainTable%
HKR,MIXER,DigitalGainTable,,%DigitalGainTable%
HKR,MIXER,SynthGainTable,,%SynthGainTable%
HKR,MIXER,Dac2GainTable,,%Dac2GainTable%
HKR,MIXER,MicGainTable,,%MicGainTable%
HKR,MIXER,MonoGainTable,,%MonoGainTable%
HKR,MIXER,DACGainTable,,%DACGainTable%
HKR,MIXER,MasterInGainTable,,%MasterInGainTable%
HKR,MIXER,MasterOutGainTable,,%MasterOutGainTable%
HKR,MIXER,Mode3MasterOutGainTable,,%Mode3MasterOutGainTable%

;-----------added this varible to enable/disable DSP serial port
HKR,MIXER,EnableDSPSerialPort,,0
;-----------added this varible to gang the same volume slider on both record--
;-----------and playback panel------------------------------------------------
HKR,DRIVER,GangLineChange,%REG_DWORD%,0x0
HKR,DRIVER,GangVolumeChange,%REG_DWORD%,0x1
;-----------------------------------------------------------------------------

;
; These values have been modified to enable/disable specific functionality
;
HKR,DRIVER,Flag_ShowRestartPanel,%REG_DWORD%,0x1
HKR,DRIVER,Flag_UseConfigurationPanel,%REG_DWORD%,0x1
; Codec_Duplex: 0 = Half, 1 = Full, 2 = Enhanced
HKR,DRIVER,Codec_Duplex,%REG_DWORD%,0x1
HKR,DRIVER,HighPassFilter,%REG_DWORD%,0x0
HKR,DRIVER,DITHER,%REG_DWORD%,0x1
HKR,DRIVER,SingleDMA,%REG_DWORD%,0x0
HKR,DRIVER,CS_GameEnable,%REG_DWORD%,0x1
HKR,DRIVER,CS_Mpu401Enable,%REG_DWORD%,0x1
HKR,DRIVER,Flag_RegistryValid,%REG_DWORD%,0x1
HKR,DRIVER,Flag_MPU401Disable,%REG_DWORD%,0x1

;
; Uncomment the following lines to enable specific functionalities
;
;HKR,DRIVER,Flag_UseConfigurationPanel,%REG_DWORD%,0x1
;HKR,DRIVER,Flag_ControlBaseAfterWSSBase,%REG_DWORD%,0x1
;HKR,DRIVER,Flag_UseRegistryOnBoot,%REG_DWORD%,0x0
;HKR,DRIVER,Flag_IgnorePnPISA,%REG_DWORD%,0x0
;HKR,DRIVER,Flag_ChangeResources,%REG_DWORD%,0x0
;HKR,DRIVER,Flag_NT351WSSBase,%REG_DWORD%,0x1
;HKR,DRIVER,CS_GameEnable,%REG_DWORD%,0x1
;HKR,DRIVER,CS_Mpu401Enable,%REG_DWORD%,0x1
;HKR,DRIVER,CS_CdRomEnable,%REG_DWORD%,0x1
;HKR,DRIVER,CS_Logical5Enable,%REG_DWORD%,0x1


HKR,CONTROLS,BoolTrue,,ON,YES,TRUE,1
HKR,CONTROLS,BoolFalse,,OFF
HKR,CONTROLS,ShortNameLine,,%SMixCtrlSynth%
HKR,CONTROLS,LongNameLine,,%LMixCtrlSynth%
HKR,CONTROLS,ShortNameAux2,,%SMixCtrlCD%
HKR,CONTROLS,LongNameAux2,,%LMixCtrlCD%
HKR,CONTROLS,ShortNameMono,,%SMixCtrlSpkr%
HKR,CONTROLS,LongNameMono,,%LMixCtrlSpkr%
HKR,CONTROLS,ShortNameMic,,%SMixCtrlMic%
HKR,CONTROLS,LongNameMic,,%LMixCtrlMic%
HKR,CONTROLS,ShortNameLoopback,,%SMixCtrlLoop%
HKR,CONTROLS,LongNameLoopback,,%LMixCtrlLoop%
HKR,CONTROLS,SourceForLine,,Synthesizer
HKR,CONTROLS,SourceForAux1,,Auxiliary
HKR,CONTROLS,SourceForAux2,,CompactDisc
HKR,CONTROLS,SourceForMono,,PCSpeaker
HKR,CONTROLS,SourceForMic,,Microphone
HKR,CONTROLS,LongNameLineOut,,%LMixCtrlMaster%
HKR,CONTROLS,ShortNameLineOut,,%SMixCtrlMaster%
HKR,CONTROLS,LongNameMuxOut,,%LMixCtrlMux%
HKR,CONTROLS,ShortNameMuxOut,,%SMixCtrlMux%
HKR,CONTROLS,LongNameLowPriMuxOut,,%LMixCtrlLowPri%
HKR,CONTROLS,ShortNameLowPriMuxOut,,%SMixCtrlLowPri%
HKR,CONTROLS,ShortNameWave,,%SMixCtrlWave%
HKR,CONTROLS,LongNameWave,,%LMixCtrlWave%
HKR,CONTROLS,ShortNameMonitor,,%SMixCtrlMonitor%
HKR,CONTROLS,LongNameMonitor,,%LMixCtrlMonitor%
HKR,CONTROLS,LongNameKaraoke,,%LMixCtrlKaraoke%
HKR,CONTROLS,ShortNameKaraoke,,%SMixCtrlKaraoke%
HKR,CONTROLS,LongNameSysVol,,%LCtrlSysVol%
HKR,CONTROLS,ShortNameSysVol,,%SCtrlSysVol%
HKR,CONTROLS,LongNameMicBoost,,%LMixCtrlMicBoost%
HKR,CONTROLS,ShortNameMicBoost,,%SMixCtrlMicBoost%

; mahler support
HKR,CONTROLS,LongNameDac2,,%LMixCtrlDac2%
HKR,CONTROLS,ShortNameDac2,,%SMixCtrlDac2%
HKR,CONTROLS,LongNameDac2Mux,,%LMixCtrlDac2Mux%
HKR,CONTROLS,ShortNameDac2Mux,,%SMixCtrlDac2Mux%

HKR,CONTROLS,LongNameZVPORT,,%LMixCtrlZVPORT%
HKR,CONTROLS,ShortNameZVPORT,,%SMixCtrlZVPORT%

HKR,CONTROLS,LongName3DEffects,,%LMixCtrl3DEffects%
HKR,CONTROLS,ShortName3DEffects,,%SMixCtrl3DEffects%


;
; These controls are used to disable XCTLs when a device
; has internal 3D circuitry.  This is to support customers
; that use XCTLs to control external SRC circuitry.
;
HKR,CONTROLS,ShortNameAux1,,%SMixCtrlAux1%
HKR,CONTROLS,LongNameAux1,,%LMixCtrlAux1%

; specification of mode2 source lines that should be usable has changed to
; a bit map, with '1' representing available and '0' representing not available.
; The bit positions represent the lines indicated by the old-style setting.
; For Playback, bit[0] (leftmost bit) == "Wave"
;               bit[1]                == "Monitor"
;               bit[2]                == "Mono"
;               bit[3]                == "Line"
;               bit[4]                == "Aux1"
;               bit[5]                == "Aux2"
; For Record,   bit[0] (leftmost bit) == "Line"
;               bit[1]                == "Aux1"
;               bit[2]                == "MixOut" (Loop)
;               bit[3]                == "Mic"
; used to be:
;HKR,CONTROLS,MixerSources,,"Wave,Monitor,Mono,Line,Aux1,Aux2"
;HKR,CONTROLS,InputSources,,"Line,Aux1,Loop,Mic"
; now is
HKR,CONTROLS,MixerSources,,111111
HKR,CONTROLS,InputSources,,1111

;----------------  controls, lines added for symmetrical mixer -----------
; for Mode3xxxSources, values are a bit map determining which source lines are
; supposed to be supported. For Mode3MixerSources, the possibilities are:
;   playback:  3D,DIG-SER,DIG-wave,DIG-synth,aux2,aux1,line-in,mic,mono
;   record:     x,DIG-SER,DIG-wave,DIG-synth,aux2,aux1,line-in,mic,x
; where x is just a placeholder to make the strings the same length and easier
; to modify correctly. Note that if line-in is set to 0, it will be ganged 
; with the DIG-synth source.
HKR,CONTROLS,Mode3MixerSources,,111111011
HKR,CONTROLS,Mode3InputSources,,x1111101x

HKR,CONTROLS,ShortName3DSpace,,%SMixCtrl3DSpace%
HKR,CONTROLS,LongName3DSpace,,%LMixCtrl3DSpace%
HKR,CONTROLS,ShortName3DCenter,,%SMixCtrl3DCenter%
HKR,CONTROLS,LongName3DCenter,,%LMixCtrl3DCenter%
HKR,CONTROLS,ShortName3DMute,,%SMixCtrl3DMute%
HKR,CONTROLS,LongName3DMute,,%LMixCtrl3DMute%
HKR,CONTROLS,ShortNameDacSER,,%SMixCtrlDacSER%
HKR,CONTROLS,LongNameDacSER,,%LMixCtrlDacSER%
HKR,CONTROLS,ShortNameLine-in,,%SMixCtrlLine%
HKR,CONTROLS,LongNameLine-in,,%LMixCtrlLine%
HKR,CONTROLS,ShortNameMonoOutMute,,%SMixCtrlMonoOutMute%
HKR,CONTROLS,LongNameMonoOutMute,,%LMixCtrlMonoOutMute%

;---------------- Setup property pannel controls ------------------------

HKR,CONTROLS,NameTitleProp,,%TitlePropSheet%
HKR,CONTROLS,NameLblIo,,%PropCtrlIo%
HKR,CONTROLS,NameLblIrq,,%PropCtrlIrq%
HKR,CONTROLS,NameLblDma,,%PropCtrlDma%
HKR,CONTROLS,NameLblPlay,,%PropCtrlPlay%
HKR,CONTROLS,NameLblCapt,,%PropCtrlCapt%

HKR,CONTROLS,NameTabLegal,,%PropCtrlTabLegal%

HKR,CONTROLS,NameTabDev0,,%PropCtrlTabDev0%
HKR,CONTROLS,NameLblWss,,%PropCtrlWss%
HKR,CONTROLS,NameLblSb,,%PropCtrlSb%
HKR,CONTROLS,NameLblSyn,,%PropCtrlSyn%

HKR,CONTROLS,NameTabDev1,,%PropCtrlTabDev1%
HKR,CONTROLS,NameLblJoy,,%PropCtrlJoy%

HKR,CONTROLS,NameTabDev2,,%PropCtrlTabDev2%
HKR,CONTROLS,NameLblBase,,%PropCtrlBase%

HKR,CONTROLS,NameTabDev3,,%PropCtrlTabDev3%
HKR,CONTROLS,NameLblMpu,,%PropCtrlMpu%

HKR,CONTROLS,NameTabDev4,,%PropCtrlTabDev4%
HKR,CONTROLS,NameLblDev4,,%PropCtrlDev4%

HKR,CONTROLS,NameTabDev5,,%PropCtrlTabDev5%
HKR,CONTROLS,NameLblDev5,,%PropCtrlDev5%

HKR,CONTROLS,JoystickRate,,0
;---------------- end of controls ---------------------------------------

HKR,DRIVER,PollHWMasterVol,,OFF
HKR,DRIVER,PowerDownBach,,OFF
HKR,DRIVER,ExternalAmpAPM,,OFF

[CWB3DSnd.AddReg]
HKLM,SOFTWARE\Crystal\CW3DSnd\Preset1,Description,,%Preset1%
HKLM,SOFTWARE\Crystal\CW3DSnd\Preset1,Center,,12
HKLM,SOFTWARE\Crystal\CW3DSnd\Preset1,Space,,4
HKLM,SOFTWARE\Crystal\CW3DSnd\Preset2,Description,,%Preset2%
HKLM,SOFTWARE\Crystal\CW3DSnd\Preset2,Center,,4
HKLM,SOFTWARE\Crystal\CW3DSnd\Preset2,Space,,12
HKLM,SOFTWARE\Crystal\CW3DSnd\Preset3,Description,,%Preset3%
HKLM,SOFTWARE\Crystal\CW3DSnd\Preset3,Center,,8
HKLM,SOFTWARE\Crystal\CW3DSnd\Preset3,Space,,8
HKLM,SOFTWARE\Microsoft\Windows\CurrentVersion\Run,CW3DSound,,%11%CWB3DSnd.exe

[CSC0010.AddReg]
HKR,Drivers\csbase\csbase.dll,Description,,%*CSC0010.DeviceDesc%

[CSBASE.AddReg]
HKR,Drivers\csbase\csbase.dll,Driver,,csbase.dll
HKR,Drivers,SubClasses,,"csbase"

[CSC0003.AddReg]
;HKR,Drivers\midi\mpu401.dll,Description,,%*CSC0003.DeviceDesc%

[MPU401.AddReg]
;HKR,Drivers\midi\mpu401.dll,Driver,,mpu401.dll
;HKR,Drivers,SubClasses,,"midi"

[MSJSTICK.AddReg]
HKR,Drivers\jport\joyport.dll,Description,,%*PNPB02F.DeviceDesc%
HKR,Drivers\jport\joyport.dll,Driver,,joyport.dll
HKR,Drivers,SubClasses,,"jport"

;
; Localizable text.
;
[Strings]
MSFT = "Microsoft"
CRYSTAL = "Crystal"
MediaClassName = "Audio-, Video- und Spiele-Controller"
CSMfgName = "Crystal Semiconductor"
DiskId = "Crystal Semiconductor Treiberdiskette"
REG_DWORD             = 0x00010001

*CSC0000.DeviceDesc = "Crystal Semiconductor CS423X Plug and Play"
*CSC0010.DeviceDesc = "Crystal Semiconductor Steuerungsbasis"
V_INTERNAL = "Crystal Semiconductor Stereo-Musik-Synthesizer"
*CSC0003.DeviceDesc = "Crystal Semiconductor MPU-401"
*PNPB02F.DeviceDesc = "Microsoft Joystick-Anschluß-Aktivierung"

cwbaudio.SvcDesc = "Crystal Semiconductor Audiotreiber"
csbase.SvcDesc = "Crystal Semiconductor Steuerungsbasis-Treiber"
joyport.SvcDesc = "Microsoft Joystick-Anschlußtreiber"

SMixCtrlSynth="Synth"
LMixCtrlSynth="Synth"
SMixCtrlLine="Direkt"
LMixCtrlLine="Direkt"
SMixCtrlCD="CD"
LMixCtrlCD="CD"
SMixCtrlSpkr="PC-Lautspr"
LMixCtrlSpkr="PC-Lautsprecher"
SMixCtrlMic="Mikr"
LMixCtrlMic="Mikrophon"
SMixCtrlLoop="MixOut"
LMixCtrlLoop="Mixer Ausgang"
SMixCtrlMaster="Master"
LMixCtrlMaster="Master Ausgang"
SMixCtrlMux="WaveIn"
LMixCtrlMux="Wave Eingang"
SMixCtrlLowPri="Neben-Ein"
LMixCtrlLowPri="Neben-Eingang"
SMixCtrlKaraoke="Karaoke"
LMixCtrlKaraoke="Karaoke Modus"
SMixCtrlX0="XCTL 0"
LMixCtrlX0="XControl 0"
SMixCtrlX1="XCTL 1"
LMixCtrlX1="XControl 1"
SCtrlSysVol="System LS"
LCtrlSysVol="System Laut."
SMixCtrlWave="Wave"
LMixCtrlWave="Wave"
SMixCtrlMonitor="Monitor"
LMixCtrlMonitor="Monitor"
SMixCtrlMicBoost="Mik Boost"
LMixCtrlMicBoost="Mikrophon Boost"

;mahler support
SMixCtrlDac2="Synth"
LMixCtrlDac2="Synth"

SMixCtrlDac2Mux="Dac2Mux"
LMixCtrlDac2Mux="Dac2Mux"

SMixCtrlZVPORT="ZVPort"
LMixCtrlZVPORT="ZVPort"

SMixCtrl3DEffects="3D Effekte"
LMixCtrl3DEffects="3D Effekte"


;-------------- controls added for symmetrical mixer ----------
SMixCtrl3DCenter="Zent."
LMixCtrl3DCenter="3D Zentrum"
SMixCtrl3DSpace="Umgebung"
LMixCtrl3DSpace="3D Umgebung"
SMixCtrl3DMute="Null"
LMixCtrl3DMute="3D Null"
SMixCtrl3D="3D Effekte"
LMixCtrl3D="3D Effekte"
; the aux1 input is usually tied to the line jack
SMixCtrlAux1="EingLeitung"
LMixCtrlAux1="Eingangs Leitung"
SMixCtrlMonoOutMute="MonoOut Null"
LMixCtrlMonoOutMute="PC-Lautspr. Null"
SMixCtrlDacSER="Ser."
LMixCtrlDacSER="Seriell In"
; optional names for a line-in that is not controlling synth
SMixCtrlLine-in="EingLeitung"
LMixCtrlLine-in="Eingangsleitung"

;---------------- Setup property pannel controls ------------------------

TitlePropSheet="CrystalWare(TM) Audiotreiber"

PropCtrlIo="I/O"
PropCtrlIrq="IRQ"
PropCtrlDma="DMA"
PropCtrlPlay="Play"
PropCtrlCapt="Capt."

PropCtrlTabLegal="Copyright"

PropCtrlTabDev0="WSS"
PropCtrlWss="WSS"
PropCtrlSyn="SYNTH"
PropCtrlSb="SB PRO"

PropCtrlTabDev1="Joystick"
PropCtrlJoy="Spieleanschluß"

PropCtrlTabDev2="Steuerung"
PropCtrlBase="Steuerungsanschluß"

PropCtrlTabDev3="MPU-401"
PropCtrlMpu="MPU-401"

PropCtrlTabDev4="Dev#4"
PropCtrlDev4="Dev#4"

PropCtrlTabDev5="Dev#5"
PropCtrlDev5="Dev#5"


Preset1="Vorg. 1"
Preset2="Vorg. 2"
Preset3="Vorg. 3"

;-------------- tables added for volume slide rcontrol ----------
;-----the values in the following table are editable to meet OEM needs
;-----however, there are limits for all these tables, for analog table,
;-----synth table and mic table, entries are ranged from 0 to 31, maximum
;-----entries for those tables are 32 entries, for digital table and DAC
;-----table, entries are ranged from 0 to 63, maximum entries number is 64,
;----for mono table, entries are ranged from 0 to 13, maximum entries is 16,
;----for masterin table, entries are ranged from 0 to 7, maximum entries is 16,
;----for masterout table, entries are ranged from 0 to 25, maximum entries is 16. 
AnalogGainTable="31,20,17,15,14,13,12,11,10,10,9,9,8,7,7,6,6,6,6,5,5,5,4,4,4,3,3,3,2,2,1,1"
DigitalGainTable="63,34,32,30,28,26,24,22,21,20,18,17,17,16,16,16,15,15,15,14,14,14,13,13,13,12,12,12,11,11,11,10,10,10,9,9,9,8,8,8,7,7,7,6,6,6,5,5,5,4,4,4,3,3,3,2,2,2,1,1,1,0,0,0"
SynthGainTable="31,20,17,15,14,13,12,11,10,10,9,9,8,7,7,6,6,6,6,5,5,5,4,4,4,3,3,3,2,2,1,1"
Dac2GainTable="31,20,17,15,14,13,12,11,10,10,9,9,8,7,7,6,6,6,6,5,5,5,4,4,4,3,3,3,2,2,1,1"
MicGainTable="31,30,29,28,27,26,25,24,23,22,21,20,19,18,17,16,15,14,13,12,11,10,9,8,7,6,5,4,3,2,1,0"
DacGainTable="63,34,32,30,28,26,24,22,21,20,18,17,17,16,16,16,15,15,15,14,14,14,13,13,13,12,12,12,11,11,11,10,10,10,9,9,9,8,8,8,7,7,7,6,6,6,5,5,5,4,4,4,3,3,3,2,2,2,1,1,1,0,0,0"
MonoGainTable="13,11,8,6,5,5,4,4,3,3,2,2,1,1,0,0"
MasterInGainTable="0,3,4,5,6,6,6,7"
MasterOutGainTable="0,7,10,11,12,13,14,14,15,15,16,17,17,18,19,20"
Mode3MasterOutGainTable="0,10,30,34,36,38,40,42,44,46,48,50,52,54,56,57"
