                               ES938CTL v1.10,
                       Copyright(c)1996, ESS Technology

                 Spatializer(tm) is a registered trademark
                    of Spatializer Audio Labratories Inc.

 ------------------------------------------------------------------------------

        To install this software simple copy the ES938CTL.EXE file somewhere

     onto in the path.


NOTE:        The Audio card MPU401 I/O port needs to be enabled before the

     ES938 control program can access the ES938 registers.  Please consult

     the documentation for your audio card for information on enabling the

     MPU401 I/O port.



     The following are the command line options:


ES938CTL [/P:<BaseIO>] [/S:<0-3>] [/T:<0-7>] [/B:<0-7>] [/V] [/?]
         /P - Set MPU401 Base I/O Port ( 0300, 0310, 0320, 0330 )
         /S - Set Spatializer(tm) Level (0-3)
         /T - Set Treble Level (0-7)
         /B - Set Bass Level (0-7)
         /V - Verbose Mode
         /? - Display Usage

