
8 megabyte soundset. 

The 8MB soundset is located in the soundsets directory of the installation CD.  To install the 8MB soundset in Windows 95, copy it to a directory on your system and then double click on the file. To install the soundset under Windows NT 4.0, choose add waveset from the AudioPCI driver dialog. Note that the 8MB waveset is recommended in systems with at least 64MB o f RAM.

The ENSONIQ Configuration utility includes a waveset manager and a 3D audio test. The waveset manager tool users to easily install and remove custom wavesets from their system.  The 3D audio test can be used to optimize speaker positioning as well as select the desired 3D audio mode. To access this utility, right click on the ENSONIQ mixer icon in the task bar and select ENSONIQ Configuration utility.
regarding installing the 8MB waveset.