----------------------------------------------------------------------------
                   INSTALLATION  INSTRUCTIONS OS/2 V3.0 (WARP)

NOTE: This procedure assumes you are installing from your CD-ROM to C: If this
is not the case make appropriate adjustments.

1.      Open OS/2 SYSTEM.

2.      Open COMMAND PROMPTS.

3.      Open an OS/2 WINDOW or OS/2 FULL SCREEN command session.

4.      Insert Paradise CD into your CD-ROM drive.

5.      From the OS/2 session type "CD-ROM drive: [enter]".
        Then from the CD-ROM drive: prompt type "CD \OS2\DRIVERS\DISK1 [enter].
        Then from the CD-ROM drive prompt type "PREPARE C" [enter]

        Now Shut Down your system, reboot your computer, and
        continue with step 6

6.      Open OS/2 SYSTEM.

7.      Open COMMAND PROMPTS.

8.      Open an OS/2 WINDOW or OS/2 FULL SCREEN command session.

9.      Make sure your Paradise CD is still inserted in the CD-ROM drive.

10.     From the OS/2 session type "CD-ROM drive: [enter]".
        Then from the CD-ROM drive: prompt type "CD \OS2\DRIVERS\DISK2" [enter].
        Then type "INSTALL C" [enter].


11.      From the DISPLAY DRIVER INSTALL window,
             select PRIMARY DISPLAY
             select OK.

12.      From the PRIMARY DISPLAY DRIVER LIST window,
             select P9710 Fully Integrated...
             select OK.

13.      From the SOURCE DIRECTORY window,
             make sure source directory points to location of
                  installation diskette (use Change radio button
                  to select the proper drive, if necessary)
             select INSTALL

14.      After installation is complete,
             from the DISPLAY DRIVER INSTALL pop-up window,
             select OK

15.     Shut down by selecting the Shut down button on the Launch Pad,
        and re-boot.

16.     If you want to change screen resolution then proceed with
        the appropriate Screen Resolution Modification instructions
        below.  (defaults to 640 x 480)


----------------------------------------------------------------------------
OS/2 3.0 (Warp) Resolution Modification

To change resolutions and pixel depths within the driver AFTER INSTALLATION,
take the following steps:

1.      Click your right mouse button on the OS/2 Desktop and select the
        entry "System Setup".  When the folder opens, double click on
        the SYSTEM icon.

2.      Select the Screen Resolution from among those listed, then close
        the System Settings Window by double clicking on the top-left
        corner.

(NOTE: you must shut-down using the Shut down radio button on the Launch
 pad, and re-boot before the change will actually take place)

