;************************************************************************
;*
;*  Chapter 1. How to use this patch file?
;*
;*	This file (RTSSRV.TXT) contains info. that helps you patch
;*	'RTSSRV.LAN'(v3.29) file into your own driver.
;*
;*	To generate your custom driver, please follow the steps
;*	described below:
;*
;*	a). Follow the instructions to edit the message area in each
;*	    line. Save this file when you finish editing.
;*	    ( see CHAPTER 2 for more details ! )
;*
;*	   !!! NOTE: DO NOT EDIT THE OFFSET AND LENGTH AREA !!!
;*
;*	b). Make sure that you have the following files in your working
;*	    directory:
;*
;*		RTPATCH.EXE	------->   The patch execution file
;*		RTSSRV.LAN	------->   RTL8139 server driver file
;*		RTSSRV.TXT	------->   RTSSRV.LAN patch info. file
;*
;*	c). After you decide the name for your packet driver,
;*	    simply type:
;*
;*	    > rtpatch  RTSSRV.lan  RTSSRV.txt  <put driver name here>  <?
;*
;*	   !!! NOTE: DO NOT USE THE SAME DRIVER NAME AS THE ORIGINAL
;*		     DRIVER!!!
;*
;*	d). If no error occurs, you should find your custom driver is
;*	    generated under your working directory.
;*
;*
;* Chapter 2. How to edit this file ?
;*
;*
;*	Each line in this file contains a display message info. of the
;*	driver. Each line has the same format:
;*
;*	    <offset> <length> <message>
;*	e.g.
;*	     1266      28    ) 'PCI driver for RTL8139',0dh,0ah,0h;
;*	     ----      --      ----------------------------------------
;*	       		  				     
;*	  Do not edit here!	  |				    | EOL
;*	       	      Put your own message here!	    |
;*	    (HEX)     (DEC)					delimiter
;*
;*
;*
;*	*NOTE: DO NOT EDIT THE <offset> AND <length> AREA !!!
;*
;*	*NOTE: Anything after comment character ';' will be ignored!
;*
;*	*NOTE: Always add ';'(EOL) at end of each line!
;*
;*	*NOTE: If delimiter is needed, keep delimiter intact! In this case,
;*	       leave the '0h' as the last byte.
;*
;*	*NOTE: 0H can only be added as delimiter! Message after 0H will be lost!
;*
;*	*NOTE: Total length of your message should not exceed <length>.
;*
;*	*NOTE: If you must use the comment character (;) in your message,
;*	       put 3bh instead of ';'.
;*
;*	*NOTE: Do not exceed 250 characters in each line.
;*
;************************************************************************


;************************************************************************
;	Put your driver name here  (no delimiter)
;************************************************************************


;************************************************************************
;	Put your driver title here ( delimiter is '0h')
;************************************************************************
; length of RTSSRV.LAN output in RTSSRV.DEF
1c 1	0ah;

;************************************************************************
; module name RTSSRV.LAN output in RTSSRV.DEF
1d 13	'RTSSRV.LAN',0h;    Must upuppercase

;************************************************************************
; Length of "Fast Ethernet Driver" description in RTSSRV.DEF
82 1	3bh;

;************************************************************************
; driver description in RTSSRV.DEF
83 59	'Fast Ethernet Driver for NetWare 3.1x and 4.0x            ';

;************************************************************************
; Length of copyright in RTSSRV.DEF
;     '(C) Copyright 1998 Realtek Co. All Rights Reserved.                   '
fa 1  46h

;************************************************************************
; copyright in RTSSRV.DEF
fb 70 '(C) Copyright 1998 Realtek Co. All Rights Reserved.                   '

;************************************************************************
d8 1	03h;	       Major version in RTSSRV.DEF    (Version 3.29)
dc 1	1dh;	       Minor version

;************************************************************************
e4 2	d0h,07h;       Year in HEX 07d0 H= 2000       (June 26,2000)
e8 1	06h;	      Month
ec 1	1ah;	      Day

;************************************************************************
d546  1 6;	Length of 'driver name' DriverNICShortName in RTSSRV.386
d547  8        'RTSSRV';    'driver name'

1cff  2  39h,81h;   Device ID
1cfd  2  ECh,10h;   Vendor ID

1e3e  2  39h,81h;   Device ID
1e3c  2  ECh,10h;   Vendor ID

