;************************************************************************
;*
;*  Chapter 1. How to use this patch file?
;*
;*      This file (RTSPKT.TXT) contains info. that helps you patch
;*      'RTSPKT.COM'(v3.20) file into your own packet driver.
;*
;*	To generate your custom driver, please follow the steps
;*	described below:
;*
;*	a). Follow the instructions to edit the message area in each
;*	    line. Save this file when you finish editing.
;*	    ( see CHAPTER 2 for more details ! )
;*
;*	   !!! NOTE: DO NOT EDIT THE OFFSET AND LENGTH AREA !!!
;*
;*	b). Make sure that you have the following files in your working
;*	    directory:
;*
;*		RTPATCH.EXE	------->   The patch execution file
;*              RTSPKT.COM      ------->   RTL8139(X) packet driver file
;*              RTSPKT.TXT      ------->   RTSPKT.COM patch info. file
;*
;*	c). After you decide the name for your packet driver,
;*	    simply type:
;*
;*          > rtpatch  rtspkt.com  rtspkt.txt  <put driver name here>  <Ù
;*
;*	   !!! NOTE: DO NOT USE THE SAME DRIVER NAME AS THE ORIGINAL
;*		     DRIVER!!!
;*
;*	d). If no error occurs, you should find your custom driver is
;*	    generated under your working directory.
;*
;*
;* Chapter 2. How to edit this file ?
;*
;*
;*	Each line in this file contains a display message info. of the
;*	driver. Each line has the same format:
;*
;*	    <offset> <length> <message>
;*	e.g.
;*           1266      28      'Packet driver for RTL8139(X)',0dh,0ah,'$';
;*	     ----      --      ----------------------------------------
;*	       		  				     
;*	  Do not edit here!	  |				    | EOL
;*	       	      Put your own message here!	    |
;*	    (HEX)     (DEC)					delimiter
;*
;*
;*
;*	*NOTE: DO NOT EDIT THE <offset> AND <length> AREA !!!
;*
;*	*NOTE: Anything after comment character ';' will be ignored!
;*
;*	*NOTE: Always add ';'(EOL) at end of each line!
;*
;*	*NOTE: If delimiter is needed, keep delimiter intact! In this case,
;*	       leave the '$' as the last byte.
;*
;*	*NOTE: 0H can only be added as delimiter! Message after 0H will be lost!
;*
;*	*NOTE: Total length of your message should not exceed <length>.
;*
;*	*NOTE: If you must use the comment character (;) in your message,
;*	       put 3bh instead of ';'.
;*
;*	*NOTE: Do not exceed 250 characters in each line.
;*
;************************************************************************

;************************************************************************
;       Put your Vendor ID and Device ID
;************************************************************************

6e20  2	ech,10h;   Vendor ID
6e1d  2	39h,81h;   Device ID

;************************************************************************
;       Put your Vendor ID and Device ID of CardBus
;************************************************************************

7030  2	ech,10h;   Vendor ID
702d  2	38h,81h;   Device ID

;************************************************************************
;	Put your driver name here  (no delimiter)
;************************************************************************

4c78 8 'RTSPKT',0h;
6c2b 8 'RTSPKT',20h,20h;

;************************************************************************
;	Put your driver title here ( delimiter is '$')
;************************************************************************

6c74 120 'Packet driver for Realtek RTL8139(X) PCI Fast Ethernet NIC, version 3.30',0dh,0ah,'$';
7370 120 'Copyright 2000(c), Realtek Semiconductor Inc.',0dh,0ah,0dh,0ah,'$';


