Realtek DMI 2.0 Network Adapter Instrumentation Layer
   Release note:
	This version support Microsoft Windows 95 and NT, and support
        RTL8139 chip.
   Installation:
        .Install Network adapter driver.
        .Before installation, a DMI service provider should be
         installed. The DMI service provider can be download from
         Intel web site(developer.intel.com/ial/WfM/tools/dmi20s/index.htm)
          or installed from LDCM.
        .Run setup to install Network Adapter Instrumentation Layer.
         After installation, restart your computer.

   Uninstallation:
        . From Control Pacel, select Add/Remove Programs applet.
        . At the Install/Uninstall table,Select
          'Realtek DMI Service(uninstall service before instrumentation)'
          Double-click Add/Remove.
        . Select 'Realtek DMI Service', double-cilck Add/Remove.


   Application that support MDI 2.0:
        .LDCM.
        .CA Unicenter TNG.

   Known problem:
        .Doesn't work on Win98.
        .Support only one Adapter.
