

                           Savage 4 Driver for
                       Windows 3.1 and Windows 3.11



Installation Instructions:

1. Copy all driver files to a diskette and place the diskette 
   in you're A: drive.
2. From the MS-DOS command prompt, make your \WINDOWS 
   subdirectory the default.
3. Run SETUP.
4. When SETUP displays its first panel, which describes your 
   hardware configuration, use the cursor keys to highlight the
   line describing your video DISPLAY, and press the ENTER key.
5. Scroll to the bottom of the list of installed display 
   drivers and highlight "Other."  Press Enter.
6. SETUP will ask for the location of your driver disk.  It 
   will suggest A:\ by default.  Since that's where your driver 
   disk is, press ENTER.
7. Select the combination of resolution, color depth, and font 
   size you prefer and press ENTER.
8. When SETUP completes the driver installation, start Windows.


