
               SiS 900/7016 PCI Fast Ethernet Adapter Installation 
                              for NDIS Driver

(1) Introduction
----------------
    These driver programs comply with Microsoft's NDIS v2.0.1
    specification. 


(2) Windows for Workgroup 3.11 installation instructions
-------------------------------------------------------
   1. In Windows for Workgroups, locate the Network section (the Network 
      icon). Open the Network group and double-click Network Setup.

   2. Click on the Networks... button in the Network Setup window.  
      Choose Install Microsoft Windows Network. 
   
    
   3. To install the network NIC, click the Drivers... button.

   4. In the Network Drivers window, click the Add adapter... button.

   5. From the list of network NICs, select Unlisted or Updated Network
      Adapter and then click OK.

   6. Network setup now requires the vendor-provided network driver.
      Be sure that the SiS LAN Driver is in your drive (For example,
      CD-ROM, HDD, Floppy) and type the path where NDIS2 driver is:
    
      [Drive name]:[Path]
      Floppy could be A:\NDIS2\DOS
      HDD could be C:\NDIS2\DOS
      CD-ROM may be E:\NDIS2\DOS
    
      Click OK.

   7. From the Unlisted or Updated Network Adapter screen, select SiS 
      900/7016 PCI Fast Ethernet Adapter and click OK.
    
    The Network Setup screen now lists the adapter, along with the 
    default protocol stacks:
    
    SiS 900/7016 PCI Fast Ethernet Adapter
       IPX/SPX Compatible Transport with NetBIOS
       Microsoft NetBEUI
       
   8.  Follow the rest screen instructions to complete the installation.

   9. When prompted, restart the computer.
 
(3) IBM LAN Services v4.x installation instructions
---------------------------------------------------

   1. Execute the installation program from the IBM DOS LAN SERVICES
      diskette

        a:\install

   2. From the Network card field, select
      "Network card not shown in list below...".

   3. Specify the path for the corresponding oemsetup.inf file of the OEM
      driver intended for use.  Then, press Enter. The program then
      displays the driver name.

        Ex. A:\NDIS2\DOS
            C:\NDIS2\DOS  (if driver is in HDD drive C)
            E:\NDIS2\DOS  (if driver is in CD-ROM drive E)

   4. Check that the driver configuration is correct or not.

   5. Complete the installation, restart your system to use the DOS
      LAN Services.


(4) Optional Parameters
-----------------------

    SLOT           - This parameter specifies the slot number used for
                     notifications. For PCI slot, you can specify from
                     1 to 16.

    MEDIATYPE      - This parameter specifies the media type currently used.
                     If MEDIATYPE does not specified, it will auto detect the
                     media type.

                     Parameters List:
                       AUTO       -- Auto-select media type.
                       UTP        -- 10BaseT half duplex mode.
                       UTPFULL    -- 10BaseT full duplex mode.
                       FAST       -- 100BaseT half duplex mode.
                       FASTFULL   -- 100BaseT full duplex mode.

