Note:  This readme file is for floppy diskette installation.  
For CD-ROM installation, please use README.WRI in the root directory 
of this CD-ROM disk for correct instructions.

***********************************************************************

                WINDOWS NT DRIVER SETUP INFORMATION
                               for
                    Trident 93xx/94xx/96xx Users


***********************************************************************
Windows NT Device Drivers Version 0.40                   Sept 23, 1996
***********************************************************************

Contents

1.0     Introduction
2.0     Supported Resolutions
3.0     Installation Notes for Windows NT Version 4.0

*****************************

1.0     Introduction

This Accelerate Driver runs on the following products:
     9440, 9470, 96XX, 93XX with PCI or VESA local bus.

The Graphics Device Drivers supplied here are for the Microsoft
Windows NT operating system version 4.0.

*****************************

2.0     Supported Modes

This Driver supports resolution up to 1600x1200, and color depth
up to True color (24 or 32 BPP).        


****************************

3.0     Installation Notes for Windows NT

This driver package containing:

  - TGIULNT.SYS         (Trident linear addressing video miniport driver)
  - TGIUL40.DLL         (Trident 256/64K/16M colors accelerated video display  driver)
  - TRIDENT.INF         (setup files used by Windows NT Setup program)
  - README              (This README file for Windows NT Version 4.0)

Windows NT drivers are included on Disk #2 of this package.  They are
located in the \NT40 sub-directory.

Procedure:

1. Run the Windows NT display Setup program located in the Control Panel, Main
   group.

2. Select "Change Display Type..." button from the Display Settings options.

3. Select "Change..." button from the Display Type options.

4. Select "Other..." button from the Select Device options.

5. Windows NT will prompt you for the correct path. Enter A:\NT40 if disk 2
   is loaded in drive A:.

6. Choose "Trident Accelerator" from the 
   list of drivers.

7. Restart Windows NT.  Windows NT will start up with 640x480x256 mode 
   using the Trident drivers.

8. Choose desired resulotion, color depth and refresh rate from the
   Display Setting applet, and click OK.

