@SCREEN
{
|DESCRIPTION|TVGA 16-Color Display (800x600)
|SHORT DESCR|VGA 16 color
|FILENAME|SD803.VGA
|SRC DISK|TRIDENT's GEM/3 driver disk
|FNT WILDCRD|*.VGA
|LONG DESCRP|
Choose this entry if you are using an AT or Compatible Machine
with an TVGA VGA card.  This display offers a
resolution of 800 horizontal by 600 vertical pixels.
}
{
|DESCRIPTION|TVGA 16-color Display (1024x768)
|SHORT DESCR|VGA color
|FILENAME|SD1K6.VGA
|SRC DISK|TRIDENT's GEM/3 driver disk
|FNT WILDCRD|*.VGA
|LONG DESCRP|
Choose this entry if you are using an AT or Compatible Machine
with an TVGA VGA card.  This display offers a
resolution of 1024 horizontal by 768 vertical pixels.
512K video memory is required.
}
{
|DESCRIPTION|TVGA 16-color Display (768x1024)
|SHORT DESCR|VGA color
|FILENAME|SD7X6.VGA
|SRC DISK|TRIDENT's GEM/3 driver disk
|FNT WILDCRD|*.VGA
|LONG DESCRP|
Choose this entry if you are using an AT or Compatible Machine,
with an TVGA VGA card and portrait display.  This display
offers a resolution of 768 horizontal by 1024 vertical pixels.
512K video memory is required.
}
