-------------------------- Upgrade History ------------------------------
Ver 7.10
        1. Greate changes have been made in this version. It auto detect the
supported refresh rate and mode. Then change the menu to display the supported
one. So from now on what you see is JUST what you CAN get.
        2. Merged 24bit and 32bit true color to one program.
        3. Added more refresh rate and display mode.
                53  132x25-8D    Text
                54  132x30-8D    Text
                55  132x43-8D    Text
                56  132x60-8D    Text
                5d  640X480x256i 60Hz
                7E  320X200-32K  70Hz
                70  512X480-32K  60Hz
                72  640X400-32K  70Hz
                74  640X480-32Ki 60Hz
                76  800X600-32K  56Hz
                76  800x600-32K  85Hz
                78  1024x768-32K 75Hz
                7F  320X200-64K  70Hz
                71  512X480-64K  60Hz
                73  640X400-64K  70Hz
                75  640X480-64Ki 60Hz
                77  800X600-64K  56Hz
                77  800x600-64K  85Hz
                79  1024x768-64K 75Hz
                6B  320x200-T    70Hz
                6C  640x480-Ti   60Hz
        3. Delete mode that never supported.
                640x350x2

Ver 7.01
========

        1. When the refresh rate is not support it report a error message. The
previous version just set the highest refresh rate it can reach.
        2. Added more refresh rate and display mode.
                800x600-T       85Hz
                1024x768-T      75Hz

Ver 7.00
========
        1. Split Hicolor into 32K color and 64K color two menu.
        2. Added more refresh rate and display mode.
                800x600x16      85Hz
                1280x1024x16    75Hz
                1600x1200x16i   96Hz

                640x480x256     72Hz
                1280x1024x256   75Hz
                1600x1200x256i  96Hz

                640x480x32K     60Hz
                640x480x32K     72Hz
                640x480x32K     75Hz
                640x480x32K     85Hz
                800x600x32K     60Hz
                800x600x32K     75Hz
                1024x768x32Ki   87Hz
                1024x768x32K    60Hz
                1280x1024x32K   87Hz

                640x480x64K     60Hz
                640x480x64K     72Hz
                640x480x64K     75Hz
                640x480x64K     85Hz
                800x600x64K     60Hz
                800x600x64K     75Hz
                1024x768x64Ki   87Hz
                1024x768x64K    60Hz
                1280x1024x64K   87Hz

                640x480xTrue    60Hz
                640x480xTrue    72Hz
                640x480xTrue    75Hz
                640x480xTrue    85Hz
                800x600xTrue    60Hz
                800x600xTrue    75Hz
                800x600xTrue    85Hz
                1024x768xTruei  87Hz
                1024x768xTrue   60Hz

        3. Fixed batch file can't set correct refresh rate problem.
        4. Cut 5F-HR 85Hz or 1024x768x16-NI (Not supported.)
        5. Fixed 5F-I 1024x768-16-I mode batch mode input can't set correct refresh rate
        6. Fixed mode 65 1600x1200-16i x-resolution data error.
        7. Fixed mode 62 1024x768-256 mode batch mode input can't set correct refresh rate

Ver 6.10
========
1. The new version is LCD chip capatable. When test LCD board,
   SVM will reset Main menu frame and automaticly adjust message
   display frame and message position.  Old the version will lost
   all display detail messages and guid message.

2. Increase 5F-I and 62-I mode. (Compare with SVM 6.0)

3. Add following mode & refresh rate:
   mode 5D-NI 75Hz
   mode 5D-HR 85Hz

4. Cut 64-NI 60Hz or 1280x1024x256-NI. (Not supported.)

5. Fixed following bug:
   The display and real mode dose not match when using
   mode 5F-I (1024x768x16c interlaced ) or
   mode 62-I (1024x768x256c interlaced )

Ver 6.0
=======
The display and real mode dose not match when using
mode 5F-I (1024x768x16c interlaced ) or
mode 62-I (1024x768x256c interlaced )
