**
**
**  VIA Rhine Family Fast Ethernet Adapter
**
**  PXE BOOTROM for Netware and Windows NT
**
**  v2.20  Jan , 2003
**
**

Introduction:
=============

  This document shows you how to install PXE Bootrom for PCI ethernet adapter
  in Windows NT Server 3.5, 3.51, 4.0.


Contents of the Subdirectory:
=============================

    PXE.TXT             This file.
    PXE.LOM             The bootrom binary file for Lan On Motherboard.
    PXE.NIC             The bootrom binary file for Network Interface Card.


Installation:
=============

  Before starting the installation process, make sure that the adapter
  is properly installed and configured. You can use the diagnostic program
  (A:\SETUP.EXE) to make sure your connection with the network is correct.

  This is for network boot by using PnP/BEV (BBS). Whether to boot or not 
  according IPL priority. The proiority for IPL devices is configurable by
  the user by editing the IPL Priority in BIOS setup.