601-7721-010 = BIOS 1xx = BIOS 2xx = FM2-A75MA-E35
601-7721-020 = BIOS 1xx = BIOS 2xx = FM2-A55M-E35
601-7721-080 = BIOS 1xx = BIOS 2xx = FM2-A85XMA-E35

601-7721-030 = BIOS Axx = BIOS Bxx = FM2-A55M-E33
601-7721-040 = BIOS Axx = BIOS Bxx = FM2-A55M-E23
601-7721-050 = BIOS Axx = BIOS Bxx = FM2-A55M-P33
601-7721-060 = BIOS Axx = BIOS Bxx = FM2-A75MA-P33
601-7721-070 = BIOS Axx = BIOS Bxx = FM2-A85XMA-P33

601-7721-090 = BIOS Axx = BIOS Bxx = FM2-A55M-P33
601-7721-100 = BIOS Axx = BIOS Bxx = FM2-A75MA-P33
601-7721-110 = BIOS Axx = BIOS Bxx = FM2-A85XMA-P33
---------------------------------------------------------------------------

FM2-A75MA-E35 / FM2-A55M-E35 / FM2-A85XMA-E35 (MS-7721) V2.4 BIOS Release
---------------------------------------------------------------------------

1. This is AMI BIOS release

2. This BIOS fixes the following problem of the previous version:
-  Update AGESA Code.
-  Enhanced OC Genie setting.

3. 2015/02/13

-------------------------------------------------------------------------------------------------------------------------
Note:
* Please download and execute the file in USB pen drive only.
  System will restart several times to update system BIOS with NVRAM & ROMHOLE.
  Please DO NOT remove the USB pen drive until BIOS updated successfully.
* Please make sure you have read the SOP before you update the BIOS.
* Please use Trinity CPU to update BIOS before changing to Richland CPU.
* There is no way to reflash back to BIOS version 1xx if you already updated to version 2xx.
-------------------------------------------------------------------------------------------------------------------------


[Below information is Chinese language]

A. AMI BIOS 正式發行

B. 此版本修正下列問題:
-  更新 AGESA Code. 
-  強化 OC Genie 相關設定.

C. 更新日期: 公元2015年02月13號

-----------------------------------------------------------------------------------------------------------
備註:
* 請務必將檔案下載於 USB 隨身碟中.並在 USB 隨身碟中執行.
  系統在更新完 BIOS 之後, 將會重啟幾次準備更新 NVRAM 及 ROMHOLE, 在未確認更新完成之前, 請勿移除 USB 隨身碟.
* 請在更新 BIOS 前, 務必先詳讀作業指導書.
* 請先使用 CPU Trinity 系列作 BIOS 更新, 只有在 BIOS 更新完成後才能使用 Richland CPU.
* 主機板韌體版本在更新至 v.2xx 之後, 將無法回到版本 v.1xx.
-----------------------------------------------------------------------------------------------------------