|  | Operation

Getting Started | Main | Advance | Monitor | Preference

Preference page

Prescan Image Area Auto Detection

If the Prescan Image Area Auto Detection is checked, the scanner will automatically detect the area of the image scanned and define the actual area of your scanned image in the Preview Window. This defined area will be used for the final scan. If the Prescan Image Area Auto Detection is not checked, the whole Preview Window area will be defined as the scan area.

Calibration

The preview scanned image has uneven vertical lines or incorrect color registration. Use this function to rectify the value and acquire better screen display.

Color/Gray Depth

Some application programs are not capable of processing 48-bit color and 16-bit gray image data. If you select 48/16 bits option, your scanned image may be abnormal or your system may be crashed. Please check whether your image processing program supports 48/16 bits image data. We would like to suggest that you check the 24/8 bits option. For more information about image data, refer to the user's manual of your application program.

Default Destination Setting

The Default Destination Setting area lets you set up your default printer and fax. You can select Printer and Fax in this area. However, please be aware that at least one printer or fax driver must be installed on your computer to perform this function.

To setup default printer and fax:

Press or to enter the setting.

This setting will be enabled when you designate the Printer or Fax as your scan destination.