;
; SETUP configuration file  for IBM one disk install 02/17/97
;

[Setup]
PackageName="CS4232 WSS 2.00 Windows 3.1 Software"
SetupName="CrystalWare Audio Setup"
SetupTitle="CrystalWare Setup",20
Caption="Crystal Ver. 2.00 Software"
SetupVersion="2.00"
SpaceRequired=2429040
FirstDisk=1
ConfigMode=0                              ; Configure = 0, Fixed = 1
ConfigOptions=111                         ; Off = 0, Options = 1, 2, 4, ...
Product=1                                 ; Kit type
DisplayNoPnPWarning=0                     ; No = 0, Yes = 1
EnablePnP=1                               ; No = 0, Yes = 1
InstallMPU401=1                           ; No = 0, Yes = 1

; Ex. LaunchApp=notepad.exe,"readme.txt"
LaunchApp=
LaunchSet=
LaunchSetMsg=

[KeyFiles]
DriverFile=cwbaudi3.drv
VxdFile=cwbaudix.386
IniFile=cwbaudi3.ini
FmFile=cwbfm.drv
MidiFile=mpu401.drv


[Mixer]
CWDDOSMixer="&2\cwdmix /c=13 /l=13"  

[sndsys.drv]
SingleModeDMA=0
; Generic = 0, WSS Compatible = 1
MsftHardware=0
MsftSupport=1
AutoSelect=0
MidiPlay=1
OldMSDosGameCompatibility=1
OldMSDOSGameIOAddress=220
BlasterSupport=CS4232
Duplex=Full
IOAddress=530
DMAADC=0
DMADAC=1
Interrupt=5
OEMHardware=
FMMixer=Line
CDMixer=Aux2
LineMixer=Aux1
BinFile="&2\cwdaudio.bin"

[mpu401.drv]
port=330
int=9

[cwbfm.drv]
portFM=388
int=0

[PNP]
WssIO=534
WssInt=5
WssDmaPlay=1
WssDmaCapture=0
SbIO=220
OplIO=388
OplInt=disable
GameIO=200
4232IO=538
4232Int=disable
MPU401IO=330
MPU401Int=9
CDIO=disable
CDInt=disable
CDDma=disable

[PMGroups]
AppCount=1
; path\filename,group file,group name,description,icon file,icon #
App0=&2\cw3dw31.exe,crystal.grp,"Crystal","3D Audio Control",,


[Dirs]
DirCount=3                      ; Must be >= 2
0=\windows
1=\windows\system
2=\crystal
3=

; Registration key,registration value

[Reg]
RegCount=0

; FileCount = number of files
; Filex = disk #,tgt filename,src filename,dir #,opt1,opt2,opt3
;  dir #: 0=WINDOWS, 1=WINDOWS\SYSTEM, 2=, 3=
;  opt1,opt2,opt3,opt4: b=create backup, i=immediate, v=version check, c=compression (src filename = compressed file)

[Files]
FileCount=13
File0=1,cwbaudi3.ini,r200d1.z,0,c
File1=1,cwbaudi3.drv,r200d1.z,1,c
File2=1,cwbaudix.386,r200d1.z,1,i,c
File3=1,oemsetup.inf,r200d1.z,1,c
File4=1,bwcc.dll,r200d1.z,1,c
File5=1,cwbfm.drv,r200d1.z,1,c
File6=1,midimap.cfg,r200d1.z,1,b,c
File7=1,mpu401.drv,r200d1.z,1,c
File8=1,cwdinit.exe,r200d1.z,2,i,c
File9=1,msmixmgr.dll,r200d1.z,1,c
File10=1,threed.vbx,r200d1.z,1,c
File11=1,cw3dw31.exe,r200d1.z,2,c
File12=1,cwdmix.exe,r200d1.z,2,c


[Strings]
StringCount=0
X0=

; Crystal Custom Section
;
; INI files
; Add item
; OEMx=0,ini path/filename,section,keyname,value,value,"message"
; Replace item
; OEMx=0,ini path/filename,section,keyname,old value,new value,"message"
;
; AUTOEXEC.BAT: p=path/env, s=string, r=replace
; OEMx=1,"message",<p,s,r>,"string","ref key",<BEFORE|AFTER|REPLACE|COMMAND>,"message"
;
; CONFIG.SYS: d=driver, s=string, c=command
; OEMx=2,d,device driver name,"ref key",<BEFORE|AFTER>,"message"
; OEMx=2,s,"string","ref key",<BEFORE|AFTER>,"message"
; OEMx=2,c,"string",value,"message"
; OEMMsg="message"
;
; DELETE ITEM
; OEMx=3,ini path/filename,section,keyname,value,"message"

[OEM]
OEMCount=0
OEM0=
OEMMsg=

