Available on the Web at www.gateway.com/support are the following: technical support for Gateway products, live chat with a Gateway Trusted Guide, files for downloading, and e-mail support.  

=======================
File Description: Ensoniq Audio PCI Wavetable Sound Card (1370 chipset) sound driver, version 4.05.1044
Version: 4.05.1044
Operating System: Microsoft(r) Windows(r) 95, Windows 98
Part Number: 7502533.exe
Date: 6/26/2001
=======================


Table of Contents
=======================
Overview
Installation
Removal 		
Troubleshooting
Reason for Update
Applicable Part Numbers
=======================


Overview

This is the installation procedure for the Ensoniq Audio PCI Wavetable Sound Card (1370 chipset) sound driver in Windows 95, and Windows 98.


Installation

Download the file to the desktop, and then perform the following steps. 

1.  On the desktop, double-click the 7502533.exe file.

2.  In the Win-Zip Self Extractor window, click Unzip to expand the files to C:\Cabs\7502533.

3.  Close all open programs.

4.  From the Start menu, click Run.

5.  In the Run dialog box, type: C:\Cabs\7502533\Wizard.exe.  Click OK.

6.  Follow the dialog boxes to install the driver.


Removal

1.  From the Start menu, click Run.

2.  In the Run dialog box, type: C:\Cabs\7502533\Wizard.exe.  Click OK.

3.  Follow the dialog boxes to remove the driver.


Troubleshooting

If you have difficulty during or after the driver installation, perform the following troubleshooting steps. 

1.  Verify that all cables are securely connected.  

2.  Verify that the sound card is fully seated in the PCI expansion slot.

3.  Review the preceding software installation procedure.  Ensure that you did not miss any of the steps. 


Reason for Update

To update to latest Gateway supported driver.


Applicable Part Numbers
2501218, 2501219, 2501222, 2501223, 2501495, 2501217, MBDSAC122ADWW, MBDSAC093AAWW, MBDSAC093ABWW, MBDSAC093ACWW, mbdsac093adww, MBDSAC093AEWW, MBDSAC094AAWW, MBDSAC094ABWW, MBDSAC094ACWW, mbdsac094adww, MBDSAC094AEWW, MBDSAC095AAWW, MBDSAC095ABWW,
MBDSAC095ACWW, mbdsac095adww, MBDSAC095AEWW, MBDSAC107AEWW,
MBDSAC108AAWW, MBDSAC108ABWW, MBDSAC108ACWW, mbdsac108adww, MBDSAC108AEWW, MBDSAC109AEWW, MBDSAC110AAWW, MBDSAC110ABWW, MBDSAC110ACWW, mbdsac110adww, MBDSAC110AEWW, MBDSAC117AAWW, MBDSAC117ABWW, mbdsac117adww, MBDSAC117AEWW, MBDSAC118AAWW, MBDSAC118ABWW, MBDSAC118ADWW, MBDSAC119AAWW, MBDSAC121AEWW, MBDSAC122AEWW, MBDSAC123AAWW, MBDSAC123ABWW, MBDSAC123ACWW, mbdsac123adww, MBDSAC123AEWW, MBDSAC124AAWW, MBDSAC124ABWW, MBDSAC124ACWW, mbdsac124adww, MBDSAC124AEWW, MBDSAC122ACWW, MBDSAC122ABWW, MBDSAC122AAWW, MBDSAC121ADWW, MBDSAC121ACWW, MBDSAC121ABWW, MBDSAC121AAWW, MBDSAC109ADWW, MBDSAC109ACWW, MBDSAC109AAWW, MBDSAC107ADWW, MBDSAC107ACWW, MBDSAC107AAWW, MBDSAC092AEWW, MBDSAC092ADWW, MBDSAC092ACWW, MBDSAC092ACWW, MBDSAC092ABWW, MBDSAC092AAWW, MBDSAC091AEWW, MBDSAC091ADWW, MBDSAC091ACWW, MBDSAC091ABWW, MBDSAC091AAWW, MBDSAC090AEWW, MBDSAC090ADWW, MBDSAC090ACWW, MBDSAC090ABWW, MBDSAC090AAWW, 6000708, 6000692, 6000566, 2501494