       RELEASE DOCUMENTATION
         FILE NAME  :  	REL_NT4.TXT
         TITLE      :  	NM2160 WINDOWS NT 4.0 DISPLAY DRIVERS 
         VERSION    :  	3.12
         ISSUE DATE :  	5/16/97
	 CONTENT    :	INSTALL.TXT	Driver installation procedure
			LICENSE.TXT	License Agreement file
			NEO20XX.DLL	Display driver file
			NEO20XX.SYS	Mini-port driver
			NEOFB.DLL	24-bit frame buffer driver
			NEOMAGIC.INF	Installation info file
			REL_NT4.TXT	Release note


       FUNCTIONAL SPECIFICATIONS
         Support OS     :  Microsoft Windows NT 4.0
         Display Mode   :  101   640x480  256
                           103   800x600  256
                           105  1024x768  256
                           111   640x480  64K (High Color)
                           114   800x600  64K (High Color)
			   117  1024x768  64K (High Color)
                           112   640x480  16M (True Color)
			   115   800x600  16M (True Color)
         Display Device :  TFT color LCD	VGA/SVGA/XGA
                           DSTN color LCD	VGA/SVGA/XGA
                           CRT
                           Simultaneous display (CRT + LCD)
         Function       :  Refer to Device Driver Specification v3.2 document.


       RELEASE HISTORY
          3/25/97  Version 3.11  NM2160 Windows NT 4.0 display drivers
          5/16/97  Version 3.12  NM2160 Windows NT 4.0 display drivers


       FIX/UPDATE ITEM
         1.  Fixed image corruption problem in 8 bit mode with Simplex Badge
	     design application.
	 2.  Fixed text corruption problem in Win NT(J).
	 3.  Fixed LCD/CRT hot key switching bad start address problem.
	 4.  Fixed hot key expansion mode switch detection problem.


       DEPENDENCY
         1.  Video BIOS version 0.02 or later.


       ADDITIONAL INFORMATION
         None