P9710 Windows NT 3.5 Drivers
Release Notes Version 1.00


I. Introduction:

This Windows NT 3.5 Driver is a  Multi-Resolution accelerated driver 
supporting 8, 16, 24, and 32 bpp(bits per pixel). 


II. Release Identification:

   The release is identifed by the Driver File Names and contents.

   See Section V for release contents.

II. Features and enhancements:

   Introduction:

   Features Supported:

      - Supports  PCI buses 
      - Multi-resolution support
      - 32-bit linear frame buffer addressing

   HW Acceleration used:

      - Hardware Cursor
      - Bitblt
      - Pattern Bitblt
      - TextOut
      - Raster Operations

   Resolutions Supported:

   640 x 480      8, 16, 32 bpp  (60 Hz, 72 Hz, 75 Hz), non-interlaced
   640 x 480      24 bpp         (60 Hz), non-interlaced
   800 x 600      8, 16, 32 bpp  (56 Hz, 60 Hz, 72 Hz,75 Hz), non-interlaced
   1024 x 768     8, 16 bpp      (60 Hz, 72 Hz, 75 Hz), non-interlaced
                                 (44 Hz), interlaced
   1024 x 768     32 bpp         (60 Hz, 72 Hz), non-interlaced
                                 (44 Hz), interlaced
   1280 x 1024    8 bpp          (60 Hz), non-interlaced
                                 (44 Hz), interlaced
   1280 x 1024    16 bpp         (44 Hz), interlaced
   1600 x 1200    8 bpp          (44 Hz), interlaced


III. Installation instructions

- Boot up Windows NT and log in as Administrator
- Select "Control Panel" in "Main" program group
- Select "Display" in  "Control Panel" program group
- Select "Change Display Type..." in "Display Settings"
- Select "Change" in "Display Type"
- Select "Other" in "Select Device" 
- Make sure that the Paradise CD is installed in your CD-ROM Drive:
- Type in "CD-ROM Drive:" 
- Select "OK"
- Select a Driver from the list of Drivers Displayed  
- Select "Install"
- Select "Yes" in "Installing Driver"
- Select "New" in "Windows NT Setup" and then select "Continue"
   The Driver will be loaded into the system at this point
- Select "OK" in "Installing Driver" and another "OK" to continue
- Select "Restart Now" in "Display Settings Change"
   NT will do a Shutdown and then a Restart with the newly installed Driver

IV. Know Problems and Limitations

V. Release Contents:

Date  Size  File
08/14/95 5  DISK1
08/14/95    NT97R10.DOC
08/14/95    29,610   OEMSETUP.INF
08/14/95    37,888   WD97R10.DLL
08/14/95    36,128   WD97R10.SYS
01/11/96    README.TXT



