;************************************************************************
;*
;*  Chapter 1. How to use this patch file?
;*
;*	This file (RTSODI.TXT) contains info. that helps you patch
;*	'RTSODI.COM'(v3.63) file into your own ODI driver.
;*
;*	To generate your custom driver, please follow the steps
;*	described below:
;*
;*	a). Follow the instructions to edit the message area in each
;*	    line. Save this file when you finish editing.
;*	    ( see CHAPTER 2 for more details ! )
;*
;*	   !!! NOTE: DO NOT EDIT THE OFFSET AND LENGTH AREA !!!
;*
;*	b). Make sure that you have the following files in your working
;*	    directory:
;*
;*		RTPATCH.EXE	------->   The patch execution file
;*		RTSODI.COM	------->   RTL8139 ODI driver file
;*		RTSODI.TXT	------->   RTSODI.COM patch info. file
;*
;*	c). After you decide the name for your packet driver,
;*	    simply type:
;*
;*	    > RTPATCH RTSODI.COM RTSODI.TXT  <put driver name here>  <?
;*
;*	   !!! NOTE: DO NOT USE THE SAME DRIVER NAME AS THE ORIGINAL
;*		     DRIVER!!!
;*
;*	d). If no error occurs, you should find your custom driver is
;*	    generated under your working directory.
;*
;*
;* Chapter 2. How to edit this file ?
;*
;*
;*	Each line in this file contains a display message info. of the
;*	driver. Each line has the same format:
;*
;*	    <offset> <length> <message>
;*	e.g.
;*	     1266      28      'Packet driver for RTL8129',0dh,0ah,'$';
;*	     ----      --      ----------------------------------------
;*	       		  				     
;*	  Do not edit here!	  |				    | EOL
;*	       	      Put your own message here!	    |
;*	    (HEX)     (DEC)					delimiter
;*
;*
;*
;*	*NOTE: DO NOT EDIT THE <offset> AND <length> AREA !!!
;*
;*	*NOTE: Anything after comment character ';' will be ignored!
;*
;*	*NOTE: Always add ';'(EOL) at end of each line!
;*
;*	*NOTE: If delimiter is needed, keep delimiter intact! In this case,
;*	       leave the '$' as the last byte.
;*
;*	*NOTE: 0H can only be added as delimiter! Message after 0H will be lost!
;*
;*	*NOTE: Total length of your message should not exceed <length>.
;*
;*	*NOTE: If you must use the comment character (;) in your message,
;*	       put 3bh instead of ';'. Same for (').
;*
;*	*NOTE: Do not exceed 250 characters in each line.
;*
;************************************************************************


;************************************************************************
;	Put your driver name here
;************************************************************************
d3f  1	06h;   Length of your driver name ----> 6 for "RTSODI"
d40  9 'RTSODI',0h;   maximum ---> 9 (8 for drvier name and 1 for delimiter 0h)

ccda 9 'RTSODI',0h;   maximum ---> 9 (8 for drvier name and 1 for delimiter 0h


;************************************************************************
;	Put your Vendor ID and Device ID
;************************************************************************

d414  2	39h,81h;   Device ID
d412  2	ech,10h;   Vendor ID

d42a  2	38h,81h;   Device ID  ==> for CardBus
d428  2	ech,10h;   Vendor ID


;************************************************************************
;	Put your messages here
;************************************************************************
d0e   1  2fh;
d0f   48 'Realtek RTL8139(A/B/C)/8130/810X Ethernet      ',0h; max --> 47
cc3f 143 'Realtek RTL8139(A/B/C)/8130/810X Fast Ethernet MLID   v3.64 (010816) ',0Dh,0Ah,'(c) Copyright 2001, by Realtek Semiconductor Corp. All rights reserved.',0h; max --> 137
cd94  89 'There is no RTL8139(A/B/C)/8130/810X Fast Ethernet PCI/CardBus card found !!          ',0Dh,0Ah,0h; max -->74
cee2  95 'More than 4 RTL8139(A/B/C)/8130/810X ethernet cards found. Driver will support only 4 cards.'0Dh,0Ah,0h; max--->90
