README.TXT FILE  FOR

Tseng Labs, Inc.
Tseng Labs Windows 95 Display Driver for ET6000/ET6100 chip 
(C) Copyright 1997. Tseng Labs, Inc.
All rights reserved.


DRIVER INFORMATION

                Driver Name:           Tseng Labs Windows 95 Display Driver for ET6000/ET6100 chip
                Driver Date:           7/25/97
                Driver Release:        7 
                Driver Version:        4.03.5000
                Driver Disk Contents:
	                                        TLIET600.DRV	(GDI MiniDriver)
                                                TLIET600.DLL	(DirectDraw Driver)
                                                TLIET600.VXD	(Virtual Display MiniDriver)
                                                TLIET600.INF	(Win 95 Driver Installation File)
                                                DISKT		(Install Disk Marker File)
                                                README.TXT	(This file you are reading)
                                                RELEASE.TXT	(Specific Driver information for the current  release)


SYSTEM REQUIREMENTS

	Operating System:   Windows 95 builds (950 , OSR2, OSR2.1)
	Tseng Graphics chip support:  ET6000/ET6100


DRIVER INSTALLATION PROCEDURE


I. Installing from Hardware Auto-Detect, Hardware 
    Installation Wizard, or Display Property Settings
    Page.

  1. Open "Control Panel"
  2. Open "Display"
  3. Choose the "Settings" Tab
  4. Select "Change Display Type"
  5. In the "Adapter Type" section select "Change"
  6. Select "Have Disk"
  7. Browse to floppy drive where Driver Disk is.
  8. Select "tsenget6.inf" and click "OK"
  9. In the "Select Device" window select "OK"
 10. In the "Change Display Type" window select "Close"
 11. Select "Apply" or "Close" and Restart



NOTES

* For Specific Driver information, please read the 
  "release.txt" file on this driver distribution.

* This release is numbered 4.03.5000 externally, but its
  internal version number is 4.03.00.5000.  This was done
  to be compliant with WHQL.  Do not be concerned about 
  this difference.  The last 4 digits are all that really 
  matter.
  
* This driver is compatible with ALL versions of Windows 95.
  It is also compatible with DirectX versions 2,3 and 3a.
  DirectX 1.0 is no longer supported in this driver!
  Please make sure that you have installed DirectX runtimes
  2, 3, and 3a from Microsoft to ensure compatibility.

* DirectX setup programs don't necessarily install the
  DirectVideo Dynamic Link Library (DLL) for 
  acceleration of programs which use the Video for 
  Windows(VFW) application interface.  If you want 
  support for Video for Windows playback you should 
  install the DirectVideo/DirectX 3.0 setup package 
  available on Tseng Labs Web Page:
  
   http://www.tseng.com/frames/download/directxv.exe


